The RAIDEN FTP SERVER features list

B A S I C
all modern ftp servers commands are supported including PASV , MDTM , SIZE , REST , that means server to server transfer , detailed file information , resume transfer are all supported
connection limit for normal users , anonymous users or even per IP connection limit
S E C U R I T Y
ip checking upon connection and (optionally) passive data transfer
manage multiple ftp servers with different settings (user file , virtual file system) within one RAIDEN FTP SERVER process
log system to log user's login attemps , read/write/delete actions and transfer speed on the servers
automatic ip rolling for data transfer channel for multiple ip servers (optionally)
'REAL' virtual file system support with UNIX STYLE owner/group/other permission system , and the user can NEVER know physical paths of virtual directories , a virtual directory mount point can be set to anywhere unlike other 'FAKE' virtual file systems in other Windows ftp servers
configurable data transfer channel port ranges ( ex : 200-1000 , 40000-60000 ) for each ftp server
user transfer ratio system ( ex: upload 1mb gains 3mb of downloading credits )
able to deny accesses if the client IP is not allowed , before or after the login attemp
P E R F O R M A N C E
ultra high performance almost 10000 kbytes/sec in the 100mbit LAN , outperforms Microsoft IIS , and the rest
more than 16000 kbytes/sec total throughput in the local loopback network (local server to local server FXP)
server side transfer speed calculation to let the users know the transfer speed of download and upload
configurable transfer speed limit for in or out streams for each user
able to serve more than 3000 connections gracefully (tested in our LAB)
F E A T U R E S
built in WindowsNT / 2000 service support , you can install RAIDEN FTP SERVER as service with the in package ServiceAgent application
built in ultra fast zip integrity checker (unlike the others which use external zip programs) , for checking incoming zip files , and no credit will be given to uploaders if they upload bad zips , of course
supports for multi-bytes characters such as Chinese and Japanese in path and file names ( ex: SERV-WHOM? doesn't suuport )
multiple languages interfaces choices for each user account ( ex: user A sees english and user B sees japanese )
external message files with variables for events such as CWD , GOODBYE , DOWNLOADED , UPLOADED , WELCOME , LISTED ( more than 20 available variables for displaying user's information and server's information ) , and 5 functions to show top 10 uploaders / downloaders , 10 latest directories , user's detail info , who is online ? ... click here to see the full listing .
special variables supports in virtual file system configuration file , ex : %s for user's name , which can be used to implement user's home directory service that no one else except the owner of the directory can see click here for an example . or %y for a DATE string , ex: 0721 for July 21th , and this can be used to create a link for /Today to c:\temp\0721 . see the full listing of variables , click here . and click here for an example
exrta site extension commands to allow user to see "who is online" "user's information" "mount a directory" "latest 10 directories made on server" "get any URL and save it in a directory" "type a text file" "update user's information (ip , password..)" "get server time" , "show top downloaders and uploaders " , and many more , click here for a full list